{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Sheet3"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet3","index":0,"n_rows":10,"n_cols":8,"rows_kept":10,"merged":[[0,0,0,7],[9,0,9,2],[10,0,10,7]],"flags":["formulas_cached_only"]}
["区应急管理局应急救援装备包采购需求清单"]
["序号","物资名称","参数要求","单位","数量","单价\n（元）","总价\n（元）","备注"]
[1,"安全帽","1.冲击吸收性能,按照 GB/T 2812 规定的方法测试，经高温（50℃±2℃）、低温（-10℃±2℃）、浸水（水温 20℃ ±2℃）、紫外线照射预处理后做冲击测试，传递到头模的力不应大于 4900 N，且帽壳不得有碎片脱落。 \n2.耐穿刺性能,按照 GB/T 2812 规定的方法测试，经高温（50℃±2℃）、低温（-10℃±2℃）、浸水（水温 20℃ ±2℃）、紫外线照射预处理后做穿刺测试，钢锥不得接触头模表面，且帽壳不得有碎片脱落。 \n3.侧向刚性,按照 GB/T 2812规定的方法测试，最大变形不应大于 40mm，残余变形不应大于 15mm，帽壳不得有碎片脱落。\n4.帽前贴LOGO，另配舒适型帽衬。","顶",29]
[2,"防护眼镜","镜片材质：聚碳酸酯 镜片：透明\n抗冲击性强：聚碳酸酯镜片可抗高速粒子45米/秒冲击能有效预防铁屑、灰沙、碎石等物因飞溅而引起眼部受伤。","副",29]
[3,"耳塞","材质：热塑性弹性体材质\nNRR:24分贝，SNR:25分贝，高降噪能力，质地柔软，高舒适。","副",29]
[4,"安全鞋","材质：全牛皮，加宽包头\n鞋底材质：欧标钢头+欧标钢底\n功能材质：聚氨酯双密度大底\n功能：SRC级防滑、防砸、防刺穿","双",84]
[5,"警用手电筒","三档灯光/配直充\n电池1*18650防爆锂电\n射程500米 尺寸150*35MM","把",29]
[6,"功能马甲","定制款\n材质：100%聚酯纤维YKK拉链\n反光印字","件",51]
[7,"应急救援装备包","材质：布艺，颜色：红色\n尺寸：43*33*15CM\n印LOGO+字","个",29]
["合计"]